{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["1.1. Long red por ancho y elec"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"1.1. Long red por ancho y elec","index":0,"n_rows":12,"n_cols":6,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
[]
["Red gestionada por Adif\na 31 de diciembre de 2022","Vía única\nsin electrificar","Vía única electrificada","Vía doble\nsin electrificar","Vía doble electrificada","Total"]
[]
["Ancho ibérico (1.668 mm)",4663.0789999999997,3377.1579999999999,102.818,3127.3520000000003,11270.406999999999]
["Ancho mixto (1.668/1.435 mm)",0,82.77000000000001,0,189.36999999999998,272.14]
["Ancho estándar (1.435 mm)                       ",0,463.81200000000013,0,2620.6589999999997,3084.4709999999995]
["Ancho métrico (1.000 mm) (1)",818.83100000000002,294.11499999999995,0,80.461999999999975,1193.4079999999999]
["Total",5481.91,4217.8549999999996,102.818,6017.8429999999989,15820.425999999998]
["LFP Perthus","-","-","-",19.899999999999999,19.899999999999999]
["Total (Adif - LFP Perthus)",5481.91,4217.8549999999996,102.818,6037.7429999999986,15840.325999999997]
[]
["(1) En ancho métrico se incluye Cercedilla-Cotos"]