{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["1.2. Evolución de la red"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"1.2. Evolución de la red","index":0,"n_rows":29,"n_cols":43,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
[null,2002,null,2003,null,2004,null,2005,null,2006,null,2007,null,2008,null,2009,null,2010,null,2011,null,2012,null,2013,null,2014,null,2015,null,2016,null,2017,null,2018,null,2019,null,2020,null,2021,null,2022,"Red ferroviaria de ancho ibérico y estándar"]
[]
["Vía única electrificada",3450.33,2.1826066147108358,3526.03,0.41506420656709508,3540.74,-0.27425437092902794,3530.98,0.54100051282339745,3550.18,0.50137605165658794,3568.07,-0.70690198462384224,3542.72,-0.14728678469522194,3537.4755300000002,0.19088867136711762,3544.26253,-1.5411553622901586E-2,3543.71353,-1.0521208312898835,3524.24,-0.40377499829752139,3510.0099999999993,-1.1626747502143786,3469.2,5.3557016026749835,3655,9.3023255813946548E-2,3658.4,-0.27334353815876966,3648.3999999999996,-1.9186492709053482E-3,3648.33,1.9798099404384857,3720.56,-1.3314124755413275,3671.0239999999994,1.1906214723739481,3714.732,3.3983070649511262,3840.9700000000003,"Vía única electrificada"]
[]
["Vía única sin electrificar",5475.52,-0.56889573958273099,5444.37,-0.58702843487860035,5412.41,-0.61469844302259879,5379.14,-1.2059548552370791,5314.27,-0.49941007890078604,5287.73,-0.40092818657533336,5266.53,-0.42950728468269528,5243.9098700000004,9.4338005851346551E-2,5248.8568700000005,-2.5510316496779595E-2,5247.5178700000006,-2.0090997803500699,5142.09,-0.26798441878692358,5128.3099999999995,-0.19324104822055688,5118.3999999999996,-5.4391997499218405,4840,-1.278925619834709,4778.1000000000004,-6.4879345346483319E-2,4775,5.8638743455503572E-2,4777.8,-0.77504290677717336,4740.7700000000004,-0.84224714550590818,4700.8409999999994,-1.0004380067311445,4653.811999999999,0.19912708119711908,4663.0789999999997,"Vía única sin electrificar"]
[]
["Vía doble electrificada",3138.82,16.047113246379219,3642.51,0.17872291359528614,3649.02,0.68073071674039642,3673.86,12.608264876723663,4137.07,6.5152390459914944,4406.6099999999997,3.0824148268169926,4542.4399999999996,0.19036024691574394,4551.0869999999995,11.633165878832919,5080.5225,1.7543766413788964,5169.6539999999995,0.97252156527305544,5219.93,4.4362663867139958,5451.5,-0.71906814638172989,5412.3,2.4130221901963864,5542.9,3.4278085478732123E-2,5544.8,-1.5149329101139983,5460.7999999999993,1.2635511280407741E-2,5461.49,0.29460824793234508,5477.58,3.2762643357102945,5657.0399999999991,2.0965027646967229,5775.6399999999994,-0.47837122812362054,5748.0110000000004,"Vía doble electrificada"]
[]
["Vía doble sin electrificar",43.22,0,43.22,24.571957427117084,53.84,29.476225854383344,69.709999999999994,13.914789843637942,79.41,2.1407883138143902,81.11,14.548144495130067,92.91,22.960929932192453,114.24299999999999,0,114.24299999999999,-53.695193578600005,52.9,-9.829867674858221,47.7,0,47.7,51.36268343815513,72.2,-72.1606648199446,20.100000000000001,0,20.100000000000001,2.4875621890547279,20.6,-12.378640776699029,18.05,-24.26592797783934,13.67,-1.4630577907809084E-2,13.668000000000001,0,13.668000000000001,652.25343868890832,102.818,"Vía doble sin electrificar"]
[]
["Total",12107.89,4.5212351423276953,12656.13,-9.4681055030632066E-4,12656.01,-1.8305177288002739E-2,12653.69,3.3716102587736829,13080.93,2.0046675568157202,13343.52,0.75650075739883693,13444.599999999999,1.5713160905050927E-2,13446.715400000001,4.019167757530151,13987.884899999999,0.63397279524979311,14013.785399999999,-0.69717001230647213,13933.960000000001,1.4608912326431209,14137.52,-0.46274028259554711,14072.099999999999,-0.10019826465132553,14058,-0.40261772656138817,14001.4,-0.68993100689931453,13904.8,6.2568321730793741E-3,13905.67,0.33734440699369372,13952.58,0.64499182230093766,14042.572999999997,0.82092505411934269,14157.851999999997,1.3916376580289267,14354.877999999999,"Total"]
[]
["Vía doble",3182.04,15.829153624718728,3685.73,0.4647654603022966,3702.86,1.0994204479780612,3743.57,12.632594021215038,4216.4799999999996,6.4328539445224431,4487.7199999999993,3.2896437389142053,4635.3499999999995,0.6467688524059767,4665.33,11.348296905042087,5194.7655000000004,0.5349327125545642,5222.5539999999992,0.86310261224681994,5267.63,4.3960946383857475,5499.2,-0.26731160896129325,5484.5,1.4313064089707268,5563,3.4154233327356565E-2,5564.9000000000005,-1.500476199033244,5481.4,-3.3932936840955108E-2,5479.54,0.21370407004968683,5491.25,3.2680719326200602,5670.7079999999987,2.0914496038237189,5789.3079999999991,1.06266586611045,5850.8290000000006,"Via doble"]
["Porcentaje",26.241702670896732,null,29.08073374661614,null,29.216167574429875,null,29.542783953837255,null,32.189499447664801,null,33.586897299109673,null,34.431313416427734,null,34.648560043088622,null,37.089877127292404,null,37.219454624783523,null,37.581044561489342,null,38.897911373423341,null,38.97428244540616,null,39.571774078816333,null,39.745311183167402,null,39.420919394741382,null,39.405077209512378,null,39.356520442814166,null,40.382257581997258,null,40.891146481825068,null,40.758472485798912,"Porcentaje"]
["Vía única",8925.65,0.49912331314805325,8970.1999999999989,-0.1923034046063643,8952.9499999999989,-0.48062370503575425,8909.92,-0.51257474814588866,8864.25,-9.7582987844446745E-2,8855.5999999999985,-0.52565608202718161,8809.0499999999993,-0.31631787763720665,8781.1853999999985,0.13362660581111019,8792.9193999999989,-2.1427470384738356E-2,8791.0313999999998,-1.4185070479898343,8666.33,-0.32320486295813566,8638.32,-0.5871512053269754,8587.5999999999985,-1.0782989426614904,8495,-0.68864037669217737,8436.5,-0.15527766253778452,8423.4,3.2409715791743565E-2,8426.130000000001,0.41774812399046368,8461.33,-1.0573396853686319,8371.864999999998,-3.9668580417867361E-2,8368.5439999999981,1.6192183490939556,8504.0489999999991,"Vía única"]
["Porcentaje",73.758297329103272,null,70.919266253383867,null,70.783832425570111,null,70.457216046162756,null,67.810500552335199,null,66.41310270089032,null,65.568686583572273,null,65.351439956911378,null,62.910122872707596,null,62.500407245900703,null,62.418955438510665,null,61.102088626576659,null,61.02571755459384,null,60.428225921183667,null,60.254688816832605,null,60.579080605258618,null,60.59492279048763,null,60.643479557185842,null,59.617742418002742,null,59.108853518174932,null,59.241527514201096,"Porcentaje"]
["Vía electrificada",6588.95,8.793358577618605,7168.34,0.2960239051161162,7189.56,0.20974857988527162,7204.64,6.6958238024384276,7687.05,3.7391457060901079,7974.4800000000005,1.3854194881672388,8084.96,4.2084685638532626E-2,8088.3625300000003,6.6295557105796377,8624.5850299999984,1.024930039246863,8713.3675299999995,0.35581170559682107,8744.17,2.4855417952761627,8961.5099999999984,-0.89281828620397619,8881.5,3.5624612959522608,9197.9,5.7621848465430503E-2,9203.2000000000007,-1.0213838664812442,9109.1999999999989,6.8063057129279514E-3,9109.82,0.96950323936147242,9198.14,1.4125029625554646,9328.0639999999985,1.7399966381019851,9490.3719999999994,1.0390425159308734,9588.9809999999998,"Vía electrificada"]
["Porcentaje",54.487959234332493,null,56.702432435204628,null,56.870398555784632,null,56.999816125552314,null,58.823506958201932,null,59.818643387878026,null,60.190156433378405,null,60.20597011653139,null,61.708239727144978,null,61.947972718554546,null,61.968375087553589,null,63.38813313791951,null,63.11424734048223,null,65.428225921183667,null,65.730569800162854,null,65.51119038030032,null,65.511550324436001,null,65.924295004938145,null,66.427028721873128,null,67.0325696299128,null,66.799460085972171,"Porcentaje"]
["Vía sin electrificar",5518.7400000000007,-0.5644404338671638,5487.59,-0.38887744893477683,5466.25,-0.31831694488908546,5448.85,-1.012507226295456,5393.68,-0.46053900120142099,5368.8399999999992,-0.17508437576831959,5359.44,-2.4016128550718996E-2,5358.1528700000008,9.2326593138047919E-2,5363.0998700000009,3.9342918296103591E-3,5300.4178700000002,-3.235331201303282,5189.79,-0.26552134094059454,5176.0099999999993,0.28187735340543441,5190.5999999999995,-6.3672793126035288,4860.1000000000004,-1.2736363449311625,4798.2000000000007,-5.4186986786717739E-2,4795.6000000000004,5.2131120193479319E-3,4795.8500000000004,-0.86345486201611266,4754.4400000000005,-0.83986757641281429,4714.5089999999991,-0.99753760147663684,4667.4799999999987,2.1085682209672285,4765.8969999999999,"Vïa sin electrificar"]
["Porcentaje",45.512040765667514,null,43.297567564795379,null,43.129601444215368,null,43.000183874447693,null,41.176493041798075,null,40.181356612121967,null,39.809843566621609,null,39.794029883468617,null,38.291760272855029,null,38.052027281445461,null,38.031624912446411,null,36.611866862080475,null,36.88575265951777,null,34.57177407881634,null,34.269430199837167,null,34.48880961969968,null,34.488449675563999,null,34.075704995061848,null,33.572971278126879,null,32.967430370087207,null,33.200539914027836,"Porcentaje"]
["Total ancho ibérico",11629.875,2.5279721407089895E-3,11630.169,-1.0317992799602216E-3,11630.048999999999,-0.22792681269012682,11603.540999999999,1.9301521837170155,11827.507,0.21433088139368728,11852.857,-5.8829698190066004E-2,11845.884,-5.0634465101973003E-2,11839.885899999999,0.10227294504587814,11851.9949,-7.3377059714552217E-3,11935,-1.3206671478643273,11779,-1.3335597249342044,11621.92,9.8778859259041951E-2,11633.4,-1.3985593205769504,11470.7,-0.5283025447444345,11410.1,-0.67221146177509183,11333.4,8.2058340833413013E-3,11334.33,-0.39870023195017268,11289.140000000001,-0.27670841180110983,11257.901999999998,-0.41374494110891646,11211.322999999999,0.52700292374059643,11270.406999999999,"Total ancho ibérico"]
["Porcentaje",95.909454893620179,null,91.763055925732189,null,91.737644064173494,null,91.545302279492461,null,90.269568316716814,null,88.68566601471602,null,87.968186780136776,null,87.908529313700853,null,84.02282472650441,null,84.100229716588927,null,83.933075859710129,null,82.65581460845965,null,82.669963971262277,null,74.561563162205374,null,80.809218260881877,null,80.407807079156299,null,74.133208277247775,null,73.435139927691125,null,72.794676488925319,null,71.885703037437708,null,71.239592410469868,"Porcentaje"]
["Total ancho estándar",477.815,114.6774379205341,1025.761,0,1025.761,2.3580541666138766,1049.9490000000001,19.360368932205276,1253.223,18.930389882726374,1490.463,7.2496264583555625,1598.5160000000001,0.52007612060183117,1606.8294999999996,32.913292916267743,2135.69,4.198385533480975,2136,-0.1889361897171824,2136,8.6095505617977466,2319.9,0,2319.9,11.547911547911525,2587.7999999999997,0.11979287425614871,2590.9,-0.75263421976920597,2571.3999999999996,-2.333359259537815E-3,2571.34,3.5817900394346793,2663.44,4.5516700207250551,2784.6709999999994,5.8124640217821053,2946.5289999999995,4.6815083102864463,3084.4709999999995,"Total ancho estándar"]
["Porcentaje",3.9404530306641412,null,8.093344474137476,null,8.0911866762479381,null,8.2834971310094776,null,9.5648135498529658,null,11.151969843666524,null,11.870667825131255,null,11.930352994606922,null,15.140633121614675,null,15.051369139056048,null,15.220396471376249,null,16.499272436066118,null,16.485812352100965,null,16.821154171162618,null,18.349410048300967,null,18.243478137482349,null,16.81808133093163,null,17.32550832827032,null,18.005950360297341,null,18.892802275449409,null,19.496763235073445,"Porcentaje"]
["Total ancho mixto",{"$nulls":4},21.7,0,21.7,0,21.7,0,21.7,0,21.7,0,21.7,443.77880184331798,118,2.0338983050847617,120.4,-1.3289036544850603,118.8,0,118.8,0,118.8,0,118.80000000000001,0,118.80000000000001,60.016835016834989,190.1,0,190.1,19.368753287743303,226.92000000000002,1.049268464657132,229.30099999999999,6.750515697707371,244.77999999999997,11.17738377318409,272.14,"Total ancho mixto"]
["Porcentaje",3.9404530306641412,null,8.093344474137476,null,0.17116925957857657,null,0.17120058949806671,null,0.16561813343021103,null,0.16236414161744614,null,0.16114539473195655,null,0.1611176916922239,null,0.83654215188090586,null,0.84840114435503189,null,0.84652766891362285,null,0.84491295547422518,null,0.84422367663674924,null,0.77222084996294904,null,0.84137169081715046,null,1.3487147833613577,null,1.2433662063399249,null,1.476100212451229,null,1.4826823073772599,null,1.569500975888751,null,1.7201812391145475,"Porcentaje"]
["Total ancho métrico",{"$nulls":4},1269,0,1269,0,1269,0,1269,0,1269,0,1269,0.6304176516942448,1277,-7.8308535630384313E-2,1276,0,1276,-5.4169278996865131,1206.8800000000001,0,1206.8800000000001,1.6571655839641153E-3,1206.8999999999999,0,1206.8999999999999,0,1206.8999999999999,-1.121053939845865,1193.3700000000001,5.8657415554108638E-3,1193.44,-2.6813245743539937E-3,1193.4079999999999,0,1193.4079999999999,0,1193.4079999999999,"Total ancho métrico"]
["Porcentaje",3.9404530306641412,null,8.093344474137476,null,0,null,0,null,0,null,0,null,0,null,0,null,0,null,0,null,0,null,0,null,0,null,7.8450618166690491,null,0,null,0,null,7.805344185480676,null,7.7632515315873203,null,7.7166908434000767,null,7.6519937112241312,null,7.5434631153421536,"Porcentaje"]
["Total red Adif",{"$nulls":4},13946.509999999998,-1.6634986100456217E-2,13944.189999999999,3.0639284174986301,14371.43,1.8271668163850165,14634.02,0.69071929654325004,14735.1,1.5713500417362525E-2,14737.415399999998,4.3784441334265694,15382.6849,0.55071725482720524,15467.4,-1.0189172065117589,15309.8,-0.276293615853902,15267.5,7.5192402161448513E-2,15278.98,0.68865853610647321,15384.2,-0.37376009152247036,15326.7,-0.16246158664291954,15301.8,-8.2735364466927308E-2,15289.14,0.54810146286843064,15372.940000000002,0.60067885518316189,15465.281999999996,0.8454937970093539,15596.039999999999,1.4387370127288506,15820.425999999998,"Total red Adif"]